**Test loader mode**

Send ‘A’

Timeout = 5 times

Enable button (to allow user clicks)

**Starter Operation**

File: LeftPanelViewModel.cs

StarterOperationTicks(object sender, EventArgs e)

Build Plot list querying from driver

Read channel 1, channel 2, SN, HW Rev, FW Rev, Motor status

Start ping

Start refresh parameters

Enable button (to allow user clicks)

No

Yes

**Function()**

File: Rs232Interface.cs

AutoConnect()

Perform Autobaud with 1[0]

**Function()**

File: LeftPanelViewModel.cs

AutoConnectCommand()

Disable button (to avoid user clicks)

Set all controls and indicators to default value (Empty)

Task task = new Task(Rs232Interface.GetInstance.AutoConnect);

task.Start();

**Model**

File: LeftPanelViewModel.cs

ActionCommand SetAutoConnectActionCommandCommand

{get {return new ActionCommand(AutoConnectCommand);}}

**Autobaud**

Success?

**Design**



File: LeftPanelView.xaml

Command="{Binding SetAutoConnectActionCommandCommand}"